**Non-Contact AC Voltage Detector**

**Product Code：MVD-135**

This voltage detector is intended to check for the presence of AC voltage, the presence of display radicalization, signaling the user with a LED and Buzzer on. Built-in bright flashlight with ON/OFF button and audible beeper indicator.

**Features:**

* Suitable for outlets or against wire insulation testing
* Flashing red LED light indicator
* Built-in bright flashlight with ON/OFF button

**Specifications:**

|  |  |
| --- | --- |
| Detection voltage range | 100V, AC to 1000V, AC,24V, AC to 1000V/ AC |
| Power | 3V(AAA\*2) alkaline battery |
| Operating temperature | –10°C to 50°C (14°F to 122°F) |
| Storage temperature | –10°C to 50°C (14°F to122°F) |
| Humidity | 95%(0°C to30°C (32°F to86°F)) |
| Altitude | 3000m |
| Contaminated distinction | II |
| Weight | 48.5g |